**Premium Laminate Specifications**

 Series: Solution Collection Laminate

Product: 80 hour water Resistant Laminate

Wear layer: AC 4 Residential, Heavy traffic

Core: HDF (High Density Fiberboard)

Locking system: Valinge 5G

Width: 7 3/4”or 197 mm

Thickness: ½” or 12mm

Plank lengths: 5’ or 1525 mm, micro beveled all four sides

Carton size: 19.11 sqft per crtn

Weight: 35 lbs per crtn

Finish: registered embossed

Warranty: 25 year limited residential warranty, 5 year light commercial warranty.

Finish effect: Wire Brushed

Installation method: Floating, Radiant heat approved